HPS8403F DVB-S2X Encoder Modulator

Product Overview

HPS8403F DVB-S/S2/S2X Encoder Modulator is an integrated device with multifunction. Its pluggable design makes it convenient to change encoding module (CVBS/SDI/HDMI/YPbPr…) as needed. It is also equipped with 1 channel ASI input. It outputs ASI and DVB-S/S2/S2X RF (IF Optional) in the same time.

The signal source could be from CCTV cameras, Blue-ray players and etc. It adopts user-friendly web-based operation interface to effectively manage the device and carefully protect your content with its BISS function. Featured with its high performance and low cost, HPS8403F is especially adequate for the TV station or DSNG system to encode SD/HD programs and output to uplink.

Key Features

MPEG2 SD/HD and MPEG4 SD/HD Encoding Module optional

CVBS/SDI/HDMI/YPbPr…signals in & 1*ASI in

Support DVB-S/S2/S2X RF (IF Optional) output and ASI output

LCN support (Logical Channel Number)

Output Frequency: 950-2150MHz; IF: 50-200MHz

QPSK, 8PSK, 16APSK, 32APSK, 8PSK-L, 16APSK-L, 32APSK-L Constellations

Support RF CID setting

Low latency achieved (CVBS Encoding modules excluded)

Support BISS fucntion

Support 10MHz reference clock

Support Web NMS and front panel LCD & Keyboard control

Upgrade device through web NMS

CID TEST SAMPLE ILLUSTRATION

Principle Chart

Technical Specifications

(Plan A) Single SDI Encoding Input

Video

Encoding	MPEG2; MPEG4 AVC/H.264
Input	SDI*1
Resolution	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only) 1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P 720*480_60i, 720*576_50i

Audio

encoding	MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC
Sample rate	48KHz
Bit rate	64kbps, 96kbps, 128kbps, 192kbps, 256kbps, 320kbps

(Plan B) Double SDI Encoding Input

Video

Encoding	H.264/AVC High Profile Level 4.0 (HD)
Input	SDI*2
Resolution	1920*1080_60P, 1920*1080_50P, 1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P 720*480_60i, 720*576_50i

Audio

encoding	MPEG1 Layer II (1 *Stereo or 2*Mono)
Sample rate	48KHz
Bit rate	64kbps, 96kbps,128kbps, 192kbps, 256kbps, 320kbps

(Plan C) Single HDMI Encoding Input

Video

Encoding	MPEG2; MPEG4 AVC/H.264
Input	HDMI*1
Resolution	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only) 1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P 720*480_60i, 720*576_50i

Audio

encoding	MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC
Sample rate	48KHz
Bit rate	64kbps, 96kbps,128kbps, 192kbps, 256kbps, 320kbps

(Plan D) HDMI/YPbPr/CVBS 3-in-1 Encoding Input

Video (HDMI)
Encoding	MPEG2; MPEG4 AVC/H.264
Interface	HDMI*1
Resolution	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only) 1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P
Audio (HDMI)
Encoding	MPEG1 Layer II; MPEG2-AAC; MPEG4-AAC
Interface	HDMI*1
Sample rate	48KHz
Bit rate	64/96/128/ 192/256/320kbps
Video (YPbPr/CVBS)
Encoding	MPEG2; MPEG4 AVC/H.264
Interface	YPbPr*1/CVBS *1
Resolution	CVBS: 720x576_50i (PAL); 720x480_60i (NTSC) YPbPr: 1920*1080_60i, 1920*1080_50i; 1280*720_60p, 1280*720_50P
Audio (L/R)
Encoding	MPEG1 Layer II; MPEG2-AAC; MPEG4-AAC
Interface	1*Stereo/2*mono
Sample rate	48KHz
Bit rate	64/96/128/ 192/256/320kbps

(Plan E) Single CVBS Input Encoding

Video

Encoding	Option 1: MPEG-2 MP@ML(4:2:0); Option 2: H.264 High Profile Level 3.0 (SD)
Input	CVBS*1 (BNC Type)
Resolution	720*576 (PAL), 720*480 (NTSC)

Audio

encoding	MPEG1 Layer II
Input	Unbalanced 1 stereo/2 Mono
Sample rate	48KHz
Bit rate	64kbps, 96kbps,128kbps, 192kbps, 256kbps, 320kbps

(Plan F) Dual CVBS Encoding Input

Video

Encoding	MPEG-2 MP@ML(4:2:0)
Input	CVBS*2 (BNC Type)
Resolution	720*576 (PAL), 720*480 (NTSC)

Audio

encoding	MPEG1 Layer II
Input	Unbalanced 1 stereo/2 Mono
Sample rate	48KHz
Bit rate	64kbps, 96kbps,128kbps, 192kbps, 256kbps, 320kbps

(Plan G) HDMI/SDI/YPbPr/CVBS/XLR/AES Encoding Input

Video

Encoding	MPEG-2 HD/SD or MPEG-4 AVC/H.264 HD/SD
Input	HDMI/SDI//YPbPr/CVBS/
Resolution	Input	Output	Interface Applicable
1920×1080i@60	1920×1080, 1440×1080, 1280×1080i, 960×1080i	HDMI SDI YPbPr
1920×1080i@59.94
1920×1080i@50
1280×720p@60	1280×720, 960×720p, 640×720p	HDMI SDI YPbPr
1280×720p@59.94
1280×720p@50
720×576i@50	720×576, 704×576, 640×576, 544×576, 528×576, 480×576, 352×576	SDI, CVBS
720×480i@59.94	720×480, 704×480, 640×480, 544×480, 528×480, 352×480	SDI CVBS
Bit rate	0.52 – 60.00 Mbps
Rate Control	CBR
GOP Structure	Auto, IP, IPB, IPBB, IPBBB
Aspect Ratio Chroma	4:3, 14:9 (for SD video), 16:9 (for HD video) 4:2:0, 4:2:2
Advanced Pretreatment	De-interlacing, noise reduction, sharpening

Audio

encoding	MPEG-1 Layer II, HE-AAC (v1&v2), LC-AAC, DD AC3 (2.0, 5.1 available); DD AC3 passthrough (for SDI in)
Input	2×XLR, 4×AES, 1×HDMI, 1×SDI (support maximum 4 stereos synchronous processing or one DD 5.1 CH processing)
Sample rate	48KHz
Bit rate	32Kbps~384Kbps
Low delay options	150ms, 200ms, 350ms, 650ms

Generals

Input Interface	1/2*CVBS /1*SDI /1*HDMI/1*(HDMI+YPbPr+CVBS 3-in-1) optional
Output	DVB-S/S2/S2X RF output; (IF Optional) ASI output
Modulation Section	Standard	DVB-S	DVB-S2	DVB-S2X
Outer coding	RS Coding	BCH Coding	BCH Coding
Inner coding	Convolution	LDPC Coding	LDPC Coding
Constellation	QPSK	QPSK,8PSK, 16APSK,32APSK	QPSK,8PSK, 16APSK,32APSK 8PSK-L,16APSK-L,32APSK-L
FEC/ Convolution Rate	1/2, 2/3, 3/4, 5/6, 7/8	QPSK: 1/4, 1/3, 2/5, 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10 8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10 16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10 32APSK: 3/4, 4/5, 5/6, 8/9, 9/10	QPSK: 13/45, 9/20, 11/20 8PSK: 23/36, 25/36, 13/18 16APSK: 26/45, 3/5, 28/45, 23/36, 25/36, 13/18, 7/9, 77/90 32APSK: 32/45, 11/15, 7/9 8PSK-L: 5/9, 26/45 16APSK-L: 5/9, 8/15, 1/2, 3/5, 2/3 32APSK-L: 2/3
Roll-off Factor	0.2,0.25,0.35	0.2, 0.25, 0.35	0.05, 0.10, 0.15
Symbol Rate	0.5~45Msps	0.5~40Msps (32APSK); 0.5~45Msps (16APSK/8PSK/QPSK)	0.5~40Msps(32APSK,32APSK-L); 0.5~45 Msps (16APSK/8PSK/QPSK/16APSK-L/8PSK-L)
BISS Scramble	Mode 0, mode 1, mode E
System	Local Control	LCD + control buttons
Remote Control	Web NMS
Low Latency Mode	Normal, Mode 1, Mode 2
Language	English
Physical Specification	Demission	410×460×44mm (W*L*H)
Temperature	0~45℃(operation), -20~80℃(storage)
Weight	4.5kgs
Power Supply	AC 100-240V 50/60Hz 2A